\begin{table}%t1
%\centering
\par
\caption{\label{tab:corrTau}Coefficients to use to correct the SFR derived from an observed calibration, as a function of the dust attenuation following Eq.~(\ref{eq:corrSFRTau}).}
\small \begin{tabular}{lrrrr}
\hline \hline
 Method & \multicolumn{2}{c}{CL01} & \multicolumn{2}{c}{Balmer}\\
calibration & $a$ & $b$ & $a$ & $b$\\
\hline
H$\alpha$ & $-0.45$ & $0.56$ & $-0.28$ & $0.44$\\
{[}O\noun{ii}{]} & $-0.80$ & $0.88$ & $-0.51$ & $0.75$\\
H$\beta$ & $-0.57$ & $0.70$ & $-0.37$ & $0.58$\\
{[}O\noun{ii}{]}/H$\beta$ (Eq.~(\ref{eq:SFROIIHb})) & $-0.18$ & $0.22$ & $-0.082$ & $0.14$\\
{[}O\noun{ii}{]}/H$\beta$ (Eq.~(\ref{eq:SFROIIHb2})) & $-0.34$ & $0.37$ & $-0.20$ & $0.30$\\
\hline
\end{tabular}
\end{table}