\begin{table} %%TABLE A1
\begin{table}%A.1
\par
%\centering
\par
  \caption {\label{Tab:App-Resi-Init}Parameters of the 2D current sheets simulated to determine
    the growth rates of resistive instabilities. The columns give from
    left to right the edge length of the square simulation box, the
    number of grid zones per dimension, the initial density (in units
    of $10^{13}~$g/cm$^{-3}$), the sound speed (in units of
    $10^{9}~$cm/s), the magnetic field (in units of $10^{14}~$G),
    the wavelength of the initial field, and the growth rate,
    \mbox{respectively}.  }
{ \begin{tabular}{ccccccc}
    \hline\hline
    $L$ 
    & $m_x$ 
    & $\rho_{0;13}$
    & $c_{\rm S;9}$
    & $b^x_{0;14}$
    & $a$
    & $\sigma$
    \\
    $\left[{\rm km}\right]$
    & 
    & $\left[ {\rm g~cm^{-3}}\right]$
    & $\left[ {\rm cm~s^{-1}} \right]$
    & $\left[ {\rm G} \right]$
    & $\left[{\rm m}\right]$
    & $\left[ {\rm ms^{-1}} \right]$
    \\
    \hline
    0.25
    & 50
    & 2.5
    & 3.1
    & 8
    & 125
    & 0.45
    \\
    0.25
    & 50
    & 2.5
    & 3.1
    & 16
    & 125
    & 1.6
    \\
    0.25
    & 50
    & 2.5
    & 3.1
    & 32
    & 125
    & 6.0
    \\
    0.25
    & 50
    & 2.5
    & 3.1
    & 64
    & 125
    & 32 
    \\
    0.25
    & 50
    & 2.5
    & 3.1
    & 16
    & 62.5
    & 10 
    \\
    0.25
    & 50
    & 2.5
    & 3.1
    & 32
    & 62.5
    & 23 
    \\
    0.25
    & 100
    & 2.5
    & 3.1
    & 16
    & 125
    & 0.60
    \\
    0.25
    & 100
    & 2.5
    & 3.1
    & 32
    & 125
    & 3.1 
    \\
    0.25
    & 100
    & 2.5
    & 3.1
    & 64
    & 125
    & 12 
    \\
    0.25
    & 100
    & 2.5
    & 3.1
    & 128
    & 125
    & 43
    \\
    0.25
    & 100
    & 2.5
    & 3.1
    & 16
    & 62.5
    & 3.7
    \\
    0.25
    & 100
    & 2.5
    & 3.1
    & 32
    & 62.5
    & 14
    \\
    0.25
    & 100
    & 2.5
    & 3.1
    & 64
    & 62.5
    & 50
    \\
    0.25
    & 100
    & 2.5
    & 3.1
    & 128
    & 62.5
    & 110
    \\
    0.25
    & 100
    & 0.025
    & 1.4
    & 3.2
    & 62.5
    & 25
    \\
    0.25
    & 100
    & 0.025
    & 3.1
    & 3.2
    & 62.5
    & 15
    \\
    0.25
    & 100
    & 0.025
    & 6.1
    & 3.2
    & 62.5
    & 8.0
    \\
    0.25
    & 100
    & 2.5
    & 1.4
    & 32
    & 62.5
    & 25
    \\
    0.25
    & 100
    & 2.5
    & 3.1
    & 32
    & 62.5
    & 14
    \\
    0.25
    & 100
    & 2.5
    & 1.4
    & 6.1
    & 62.5
    & 7.8
    \\
    0.25
    & 100
    & 250
    & 6.6
    & 320
    & 62.5
    & 7.4
    \\
    0.25
    & 100
    & 250
    & 3.1
    & 320
    & 62.5
    & 15
    \\
    0.25
    & 100
    & 2.5
    & 12.4
    & 64
    & 62.5
    & 16
    \\
    0.25
    & 100
    & 2.5
    & 3.1
    & 4
    & 31.25
    & 1.2
    \\
    0.25
    & 100
    & 2.5
    & 3.1
    & 8
    & 31.25
    & 5.9
    \\
    0.25
    & 100
    & 2.5
    & 3.1
    & 16
    & 31.25
    & 20
    \\
    0.25
    & 100
    & 2.5
    & 3.1
    & 32
    & 31.25
    & 53
    \\
    0.25
    & 100
    & 2.5
    & 3.1
    & 64
    & 31.25
    & 110
    \\
    0.25
    & 200
    & 2.5
    & 3.1
    & 32
    & 125
    & 0.9
    \\
    0.25
    & 200
    & 2.5
    & 3.1
    & 64
    & 125
    & 4.6
    \\
    0.25
    & 200
    & 2.5
    & 3.1
    & 128
    & 125
    & 19
    \\
    0.25
    & 200
    & 2.5
    & 3.1
    & 32
    & 62.5
    & 5.4
    \\
    0.25
    & 200
    & 2.5
    & 3.1
    & 64
    & 62.5
    & 24
    \\
    0.25
    & 200
    & 2.5
    & 3.1
    & 128
    & 62.5
    & 76
    \\
    0.25
    & 200
    & 2.5
    & 3.1
    & 16
    & 31.25
    & 7.9
    \\
    0.25
    & 200
    & 2.5
    & 3.1
    & 32
    & 31.25
    & 28
    \\
    0.25
    & 200
    & 2.5
    & 3.1
    & 64
    & 31.25
    & 95
    \\
    0.25
    & 200
    & 2.5
    & 3.1
    & 128
    & 31.25
    & 250
    \\
    0.25
    & 200
    & 2.5
    & 3.1
    & 4
    & 15.625
    & 2.5
    \\
    0.25
    & 200
    & 2.5
    & 3.1
    & 16
    & 15.625
    & 40
    \\
    0.25
    & 200
    & 2.5
    & 3.1
    & 64
    & 15.625
    & 260
    \\
    0.5
    & 100
    & 2.5
    & 3.1
    & 32
    & 250
    & 1.2
    \\
    0.5
    & 100
    & 2.5
    & 3.1
    & 64
    & 250
    & 5.6
    \\
    0.5
    & 100
    & 2.5
    & 3.1
    & 128
    & 250
    & 20
    \\
    0.5
    & 100
    & 2.5
    & 3.1
    & 16
    & 125
    & 1.9
    \\
    0.5
    & 100
    & 2.5
    & 3.1
    & 32
    & 125
    & 7.5
    \\
    0.5
    & 100
    & 2.5
    & 3.1
    & 64
    & 125
    & 26
    \\
    0.5
    & 100
    & 2.5
    & 3.1
    & 8
    & 62.5
    & 3.0
    \\
    0.5
    & 100
    & 2.5
    & 3.1
    & 16
    & 62.5
    & 10
    \\
    0.5
    & 100
    & 2.5
    & 3.1
    & 32
    & 62.5
    & 24
    \\
    0.5
    & 100
    & 2.5
    & 3.1
    & 64
    & 62.5
    & 61
    \\
    \hline 
\end{tabular}}
\end{table}