\begin{table}%t3
\caption{\label{7:tab:COprop}Properties of the $^{12}$CO lines$^a$.}
\footnotesize
%\centerline
 {\begin{tabular}{l c r r r r r r}  
\hline \hline
Source &   Offpos.  &$V_{LSR}$     & \multicolumn{5}{c}{CO 6--5}            \\
& & & \multicolumn{5}{c}{\hrulefill} \\
       &           &        & $\int T_{\rm{MB}} {\rm d}V$ & $T_{\rm{peak}}$ &  red  & blue & rms$^b$ \\ 
       &($\arcsec$, $\arcsec$)& km s$^{-1}$ & K km s$^{-1}$        & K  & \multicolumn{2}{c}{K km s$^{-1}$}  & K           \\ \hline
NGC 1333 IRAS 2    & 0, 0 & 7.0 & 34.3 & 6.8 & 8.9  & 13.2 & 0.6 \\
               & 0, 20 & 7.0 & 43.7 & 9.8 & 20.0 & --    & 0.6 \\
            & --20, --20 & 7.0 & 36.3 & 7.6 & 2.2  & 11.0 & 0.7 \\
L 1551 IRS 5    & 0, 0 & 6.8 & 39.5 & 7.8 & 13.8 & 10.7 & 0.3 \\
%             & -20,-20& 6.0 & 14.2 & 3.2 & 2.0 & 5.3   & 0.2\\
%             & 10, 20 & 6.5 & 12.3 & 3.0 & 4.2 & 1.7   & 0.2 \\
TMR 1           & 0, 0 & 4.5 & 23.4 & 8.1 & 2.5  & 5.2  & 0.3 \\ 
HH 46           & 0, 0 & 4.4 & 45.3 & 9.3 & 10.6 & 10.4 & 0.3 \\
            & --20, --20 & 4.4 & 33.4 & 9.1 & 11.1 & --    & 0.5\\
Ced 110 IRS4    & 0, 0 & 3.5  & 20.8 & 7.8  & --   & 4.8 & 0.4 \\
BHR 71          & 0, 0 & --4.5 & 38.6 & 5.2  & 9.1 & 12.7& 0.4 \\
       & 10, --40      & --4.5 & 96.3 & 16.5 & --   & 68.1& 1.0 \\
       & 0, 40        & --4.5 & 75.8 & 13.0 & 41.5& --   & 1.0 \\
IRAS 12496-7650 & 0, 0 & 1.8  & 22.1 & 5.9  &  --  & --   & 0.5 \\
RCrA IRS 7A$^c$     & 0, 0 & 5.7 & 337.9 & 36.3 & 33.6& 10.9& 0.3 \\ \hline
Source &   Offpos.  &$V_{\rm LSR}$ & \multicolumn{5}{c}{CO 7--6}  \\ 
& & &  \multicolumn{5}{c}{\hrulefill} \\ 
& & & $\int T_{\rm{MB}} {\rm d}V$ & $T_{\rm{peak}}$ & red  &  blue & rms$^b$ \\ 
 &($\arcsec$, $\arcsec$)& km~s$^{-1}$  & K km s$^{-1}$        & K             &  \multicolumn{2}{c}{K km s$^{-1}$} & K \\\hline
NGC 1333 IRAS 2    & 0, 0 & 7.0 & 29.2 & 6.3 & 8.8 & 5.2 & 1.7 \\
               & 0, 20 & 7.0 & 65.8 & 10.1& 27.8& 5.2 & 1.7\\
            & --20, --20 & 7.0 &--    & --    & --   & --   & 3.5\\
L 1551 IRS 5    & 0,0 & 6.5 & 52.9 & 9.2 & 18.9 & 11.6 & 0.4\\
%             & -20,-20& 6.0 &  8.4  & 5.2 & -   & 3.5 & 0.6\\
%             & 10, 20 & 6.5 & 12.6 & 3.4 & 5.0 & 3.2 & 0.5\\
TMR 1           & 0, 0 & 4.5 & 19.8 & 10.1& 1.5 & 1.8 & 0.7\\
HH 46           & 0, 0 & 4.4 &34.2 & 8.4 & --    & 9.9 & 0.8\\
            & --20, --20 & 4.4 & 29.8 & 6.2 & 15.7 & --   & 1.0\\
Ced 110 IRS4    & 0, 0 & 3.5  &23.1 & 7.1 & --    & --   & 1.0\\
BHR 71          & 0, 0 & --4.5 &36.6 & 4.4 & 5.4  & --   & 0.7\\
       & 10, --40      & --4.5 &41.5 & 7.0 & 5.6  &17.2 & 2.8\\
       & 0, 40        & --4.5 &54.7 & 9.1 & 27.0 & --   & 3.0\\
IRAS 12496-7650 & 0, 0 & 1.8  &19.9 & 6.1 & --    & --   & 1.4\\
RCrA IRS 7A$^c$     & 0, 0 & 5.7 &407.6& 46.3& 29.0 & 22.2& 0.7\\  
\hline 
\end{tabular}}
\par
\smallskip
\par
$^a$  Red is the redshifted outflow lobe calculated from --10 to --1.5~km~s$^{-1}$ with respect to the source velocity. Blue is the blueshifted outflow lobe calculated from +1.5 to +10~km~s$^{-1}$ with respect to the source velocity.\\
$^b$ 1$\sigma$ in a 0.8~km~s$^{-1}$ channel.\\
$^c$ Outflowing gas refers to emission in  --20 to --8~km~s$^{-1}$ and +8 to +20~km~s$^{-1}$ from line center.
\end{table}