\begin{table}%t2
\caption{\label{parameters}Input parameters ($L_\star$, $T_{\rm eff}$, $\log$(C{--}O), $P$) and the resulting avergage mass loss rate, average wind speed and the mean degree of dust condensation at the outer boundary for a subset of models with $M_\star = 1~M_\odot$ and $\Delta u_{\rm p} = 4.0~\mbox{km~s}^{-1}$.}
%\centerline
 {\small \begin{tabular}{lcccccccccccc}  
  \hline  \hline\noalign{\smallskip}
$\log(L_\star)$ & $T_{\rm eff}$  & log(C{--}O)+12 & $P$ & $\langle\dot{M}\rangle$ & $\langle u_{\rm out} \rangle$ & $\langle {\rm f_c} \rangle$ & 
$\langle {\rho_{\rm d}/\rho_{\rm g}} \rangle$ & $\langle a_{\rm gr}\rangle$\\[1mm]
[$L_{\odot}$] &  [$\mbox{K}$] & & [days] & [$M_\odot$ yr$^{-1}$] & [km~s$^{-1}$] & & & [cm]\\
\hline
3.70   & 2400   &    8.20   &   295   &  --  & -- & -- &--  &   1.26E-04  \\
3.70   & 2400   &    8.50   &   295   &   1.05E-06   &   3.80E+00   &   2.44E-01   &   6.61E-04   &   2.32E-05  \\
3.70   & 2400   &    8.80   &   295   &   3.02E-06   &   2.00E+01   &   3.19E-01   &   1.73E-03   &   1.19E-05  \\
3.70   & 2400   &    9.10   &   295   &   4.46E-06   &   3.86E+01   &   4.75E-01   &   5.13E-03   &   5.78E-06  \\
3.85   & 2400   &    8.20   &   393   &   --  &  --  &  -- &  -- &  1.08E-04  \\
3.85   & 2400   &    8.50   &   393   &   3.15E-06   &   7.76E+00   &   2.13E-01   &   5.77E-04   &   2.32E-05  \\
3.85   & 2400   &    8.80   &   393   &   5.40E-06   &   2.19E+01   &   2.85E-01   &   1.54E-03   &   1.15E-05  \\
    3.85   & 2400   &    9.10   &   393   &   7.95E-06   &   4.15E+01   &   5.24E-01   &   5.65E-03   &   6.19E-06  \\
    4.00   & 2400   &    8.20   &   524   &   2.42E-06   &   8.67E-01   &   2.54E-01   &   3.45E-04   &   8.30E-05  \\
    4.00   & 2400   &    8.50   &   524   &   8.50E-06   &   1.14E+01   &   2.15E-01   &   5.83E-04   &   2.48E-05  \\
    4.00   & 2400   &    8.80   &   524   &   1.23E-05   &   2.42E+01   &   3.36E-01   &   1.82E-03   &   1.26E-05  \\
    4.00   & 2400   &    9.10   &   524   &   1.59E-05   &   4.43E+01   &   5.88E-01   &   6.34E-03   &   6.70E-06  \\
    3.70   & 2600   &    8.20   &   295   &   -- & -- &  -- & --& --   \\
    3.70   & 2600   &    8.50   &   295   &   7.60E-07   &   6.24E+00   &   2.11E-01   &   5.72E-04   &   --         \\
    3.70   & 2600   &    8.80   &   295   &   1.95E-06   &   2.68E+01   &   4.00E-01   &   2.16E-03   &   1.41E-05  \\
    3.70   & 2600   &    9.10   &   295   &   3.96E-06   &   4.39E+01   &   5.84E-01   &   6.30E-03   &   7.38E-06  \\
    3.85   & 2600   &    8.20   &   393   &   --          &   --          &   --          &   --	      &   1.05E-04  \\
    3.85   & 2600   &    8.50   &   393   &   1.67E-06   &   6.24E+00   &   1.71E-01   &   4.63E-04   &   1.87E-05  \\
    3.85   & 2600   &    8.80   &   393   &   4.04E-06   &   2.65E+01   &   3.22E-01   &   1.74E-03   &   1.24E-05  \\
    3.85   & 2600   &    9.10   &   393   &   5.66E-06   &   4.65E+01   &   5.25E-01   &   5.67E-03   &   6.20E-06  \\
    4.00   & 2600   &    8.20   &   524   &   1.22E-06   &   1.34E+00   &   2.06E-01   &   2.80E-04   &   5.52E-05  \\
    4.00   & 2600   &    8.50   &   524   &   4.85E-06   &   1.04E+01   &   1.57E-01   &   4.26E-04   &   2.10E-05  \\
    4.00   & 2600   &    8.80   &   524   &   8.43E-06   &   2.80E+01   &   3.25E-01   &   1.76E-03   &   1.18E-05  \\
    4.00   & 2600   &    9.10   &   524   &   1.09E-05   &   4.55E+01   &   4.88E-01   &   5.27E-03   &   6.26E-06  \\
    3.70   & 2800   &    8.20   &   295   &   --          &   --          &   --          &   --	 &--         \\
    3.70   & 2800   &    8.50   &   295   &   --          &   --          &   --          &   --	      &--         \\
    3.70   & 2800   &    8.80   &   295   &   1.46E-06   &   3.00E+01   &   4.55E-01   &   2.46E-03   &   1.66E-05  \\
    3.70   & 2800   &    9.10   &   295   &   2.52E-06   &   4.10E+01   &   4.69E-01   &   5.06E-03   &   6.94E-06  \\
    3.85   & 2800   &    8.20   &   393   &   --          &   --          &   --          &   --	   &   --  \\
    3.85   & 2800   &    8.50   &   393   &   1.49E-06   &   1.71E+01   &   2.25E-01   &   6.10E-04   &   --   \\
    3.85   & 2800   &    8.80   &   393   &   2.71E-06   &   2.83E+01   &   3.15E-01   &   1.70E-03   &   1.28E-05  \\
    3.85   & 2800   &    9.10   &   393   &   4.77E-06   &   4.68E+01   &   5.14E-01   &   5.55E-03   &   7.57E-06  \\
    4.00   & 2800   &    8.20   &   524   &   -- &   -- &  --  &  --	      &   5.71E-05  \\
    4.00   & 2800   &    8.50   &   524   &   3.72E-06   &   1.31E+01   &   1.72E-01   &   4.66E-04   &   2.15E-05  \\
    4.00   & 2800   &    8.80   &   524   &   5.76E-06   &   2.81E+01   &   2.94E-01   &   1.59E-03   &   1.33E-05  \\
    4.00   & 2800   &    9.10   &   524   &   8.07E-06   &   4.96E+01   &   3.87E-01   &   4.18E-03   &   6.12E-06  \\
    3.70   & 3000   &    8.20   &   295   &   -- &  --  &  --  &  --	      &   -- \\
    3.70   & 3000   &    8.50   &   295   &   --&   -- &   -- &  --	      &   --     \\
    3.70   & 3000   &    8.80   &   295   &   --          &   --          &   --          &   --	      &   1.25E-05  \\
    3.70   & 3000   &    9.10   &   295   &   5.50E-07   &   3.09E+01   &   2.84E-01   &   3.06E-03   &   4.79E-06  \\
    3.85   & 3000   &    8.20   &   393   &   --          &   --          &   --          &   --	&   --         \\
    3.85   & 3000   &    8.50   &   393   & -- &--&--&--&-- \\
    3.85   & 3000   &    8.80   &   393   &   1.47E-06   &   3.12E+01   &   3.76E-01   &   2.03E-03   & -- \\
    3.85   & 3000   &    9.10   &   393   &   3.62E-06   &   4.27E+01   &   4.25E-01   &   4.59E-03   &   6.55E-06  \\
    4.00   & 3000   &    8.20   &   524   & -- & -- & --&-- &--   \\
    4.00   & 3000   &    8.50   &   524   &   1.72E-06   &   1.83E+01   &   1.75E-01   &   4.74E-04   &   2.66E-05  \\
    4.00   & 3000   &    8.80   &   524   &   3.85E-06   &   2.73E+01   &   2.86E-01   &   1.55E-03   &   1.21E-05  \\
    4.00   & 3000   &    9.10   &   524   &   8.00E-06   &   4.76E+01   &   5.56E-01   &   6.00E-03   &   7.43E-06  \\
    3.70   & 3200   &    8.20   &   295   &-- & -- & --  & --  & --     \\
    3.70   & 3200   &    8.50   &   295   & --  &  -- &   --        & --   &  --  \\
    3.70   & 3200   &    8.80   &   295   &--  & --   & --  & --      &  --         \\
    3.70   & 3200   &    9.10   &   295   &   1.13E-06   &   4.56E+01   &   3.22E-01   &   3.47E-03   &   5.64E-06  \\
    3.85   & 3200   &    8.20   &   393   &  --  & --  &-- &  --      & --        \\
    3.85   & 3200   &    8.50   &   393   & --  &  --& -- &  --   & --      \\
    3.85   & 3200   &    8.80   &   393   & --  &--  & --   & --      &   --        \\
    3.85   & 3200   &    9.10   &   393   &   5.17E-07   &   3.98E+01   &   2.77E-01   &   2.99E-03   &   5.03E-06  \\
    4.00   & 3200   &    8.20   &   524   &  --      &  -- &  --   &   --	      &--         \\
    4.00   & 3200   &    8.50   &   524   & -- & -- & -- & -- &--     \\
    4.00   & 3200   &    8.80   &   524   &   1.64E-06   &   3.33E+01   &   3.09E-01   &   1.67E-03   &   1.47E-05  \\
    4.00   & 3200   &    9.10   &   524   &   3.68E-06   &   5.10E+01   &   3.65E-01   &   3.94E-03   &   5.75E-06\\
  \hline
  \end{tabular}}
\medskip
The dust-to-gas mass ratio $\rho_{\rm d}/\rho_{\rm g}$ is calculated from $f_{\rm c}$ as described in H\"ofner \& Dorfi (1997) and  the grain radius is defind as $a_{\rm gr}=r_0~(K_1/K_0)$, where $K_0, K_1$ are the zeroth and first moment of the grain-size distribution, 
respectively. Models with $\log$(C--O)+12~=~7.90 are not included, since none of them produced any outflow.
    \end{table}