Fig. 3. Identification of the He and metallic lines used for spectral classification in IGR J06074+2205 (middle spectrum). A comparison with two MK standards is provided: the B0V ffl Per (top) and the B1V 42 Ori (bottom).