(a) FLD run at t = 44 kyr (b) RT+FLD run at t = 39 kyr

(c) FLD run at t = 49 kyr (d) RT+FLD run at t = 44 kyr

(e) FLD run at t = 54 kyr (f) RT+FLD run at t = 49 kyr