(a) Force accuracy as a function of the opening angle `_{crit}. (b) Force accuracy as a function of the computation time.