(a) 35 to 55 km s^{�1} component peak velocity

(b) 35 to 55 km s^{�1} component line width

(c) 65 to 78 km s^{�1} component peak velocity

(d) 65 to 78 km s^{�1} component line width