(a) 35 to 55 km s^{�1} component at a distance of 4 and 12 kpc.

(b) 65 to 78 km s^{�1} component at a distance of 4.5 kpc.

(c) 78 to 120 km s^{�1} component at a distance of 5 to 7 kpc.