0.5 1 1.5 2 2.5 3 3.5 4 x 10^4 -3

-2

-1

0

1

2

3

Residual visibility phase (rad)

Calibrated visibility power (arbit.)

Residual visibility phase, ~60 MHz