-25 -20 -15 -10 -5 0 -10

-5

0

5

10

z [Mm]

Averaging kernel [Mm -1]

1.9 Mm

ridge component phase-speed component sum